Project title: ハートフル成田東

建物名称：ハートフル成田東

所在地：東京都杉並区成田東3-26-6

主要用途：児童福祉施設等(老人ホーム)

※地域密着ユニット型特別養護老人ホーム(29床)

※地域密着型小規模多機能居宅介護施設(9床)

建築主：社会福祉法人　愛あい会

設計：アプルデザインワークショップAPLdw

担当/大野秀敏、江口英樹、山本真也、罍彩子(\*)(\*\*)、劉ジェシー(\*)(\*\*)

(\*)元所員、(\*\*)工事監理担当者

構造設計：小西泰孝建築構造設計　担当：小西泰孝

設備設計：総合設備計画　担当：吉岡聡史　兵道哲

施工：松井建設　担当：穗積寿和

構造・構法：鉄骨造

階数：地上2階

軒高：6.38m　最高の高さ：9.25m

敷地面積：1635.94m2

建築面積：807.90m2（建蔽率49.38% 許容50%）

延床面積：1428.76m2（容積率66.51% 許容100%）

1階：771.83m2

2階：656.93m2

設計期間：2017年8月〜2018年12月

工事期間：2019年1月〜2019年11月

地域地区：第一種低層住居線表地域、準防火地域、第一種高度地区

道路幅員：東3.5-3.8m　南3.0-3.5m 西3.8-4.0m

# 撮影：北嶋俊治

Location: Suginami-ku, Tokyo, Japan

Completion date: 2019.11

Client: Aiaikai, Social welfare corporation

Architect: A.P.L. design workshop. OHNO, Hidetoshi, EGUCHI, Hideki, YAMAMOTO, Shinya,

Structural engineering: Konishi Structural Engineers

Mechanical and Electrical engineer: SOGOCONSULTANTS. (MECHANICAL&ELECTRICAL ENGINEERSASSOCIATE)

Contracotrs: Matsui Kensetsu K.K.

Site area：1635.94㎡

Floor area：1F:771.83㎡ 2F: 656.93m2

Photo: kitajima toshiharu/archi photo